{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["设备采购清单"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"设备采购清单","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"merged":[[0,0,0,4],[2,5,4,5]]}
["设备采购需求清单"]
["序号","产品名称","技术规格","单位","数量"]
[1,"全彩高清摄像头\n（枪机：室外）","①12V电源供电摄像机；\n②分辨率达1920 × 1080 @25 fps及以上，在该分辨率下可输出实时图像；\n③焦距4mm；\n④像素400万；\n⑤带全彩夜视、拾音功能。","台",68]
[2,"全彩高清摄像头\n（半球：室内）","①POE供电摄像机\n②分辨率达1920 × 1080 @25 fps及以上，在该分辨率下可输出实时图像；\n③焦距2.8mm；\n④像素400万；\n⑤带全彩夜视、拾音功能。","台",367]
[3,"全彩高清警戒摄像头（枪机：周界、天台）","①12V电源供电摄像机\n②分辨率达1920 × 1080 @25 fps及以上，在该分辨率下可输出实时图像；\n③焦距4mm；\n④像素400万；\n⑤带全彩夜视、远程喊话、拾音功能。","台",19]
[4,"网线","6类及以上无氧铜芯丝","米",25220]
[5,"电源适配器","12V/2A监控专用","个",96]
[6,"电源线","2*1.5护套线","米",4030]
[7,"16口千兆POE交换机","16个千兆网口、2个千兆光口交换机容量不低于36Gbps，包转发率不低于20Mpps。","台",8]
[8,"8口千兆POE交换机","8个千兆网口交换机容量不低于20Gbps，包转发率不低于14Mpps。","台",79]
[null,"24口千兆POE交换机","24个千兆网口、4个千兆光口交换机容量不低于2Tbps，包转发率不低于200Mpps","台",4]
[9,"8口千兆普通电源\n交换机","8个千兆网口交换机容量不低于20Gbps，包转发率不低于14Mpps。","台",43]
[12,"收发器","千兆单模双纤","对",20]
[15,"监控立杆","铁质，2.0厚，高3米，横臂0.8米，3机位","根",22]
[16,"室外汇聚箱","全铁质，铁皮厚度不低于1.0mm,尺寸：高40cm、宽30cm、深20cm","个",27]
[17,"室内汇聚箱","全铁质，铁皮厚度不低于1.0mm,玻璃门，尺寸：高30cm、宽53cm、深40cm","个",34]
[18,"片区汇聚箱","铝合金材质，厚度不低于1.0mm，尺寸：高130cm、宽80cm、深60","个",1]
[19,"监控设备授权","监控设备信号回传","路",1000]
[20,"电脑主机","主板、显卡：近两年上市品牌主流产品，拓展性和兼容性极强；CPU：12核，运行内存：不低于16GB；硬盘：机械硬盘不低于4TB,固态硬盘不低于512GB；电源功率不低于700W；能够承受长时间运行，使用寿命长，带刻录光驱，机箱内独立散热风扇。","台",7]
[21,"摄像机支架","吊装/壁装/立杆安装，万向调节，铝合金材质。","个",87]
[22,"光纤","8芯电信级","米",2700]
[23,"辅材","终端盒、PVC线管1批（含接头）、跳线、光模块、水晶头、法兰头、插线板、项目建设其他所需辅材以及设备安装调试","批",1]