{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["新增购买仪器设备"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"新增购买仪器设备","index":0,"n_rows":4,"n_cols":7,"rows_kept":4,"merged":[[0,0,0,6],[3,0,3,2]]}
["新增购买仪器设备项目"]
["序号","院校需求部门","项目名称","项目设备清单及价格","总额（万元）","基本性能","备注"]
[1,"建筑工程学院","全站仪","全站仪8套",null,"（1）测角精度：≤2″；\n（2）最小读数：1″；\n（3）棱镜测程：≥5000m；\n（4）测距精度：2mm+2ppm；\n（5）免棱镜测程：1000m；\n（6）免棱镜精度：3mm+2ppm\n（7）补偿器：补偿范围±3′，精度1″；\n（8）支持摄像辅助放样、桥梁功能、隧道功能、CAD放样、点之记功能，可自动计算仪器高；\n（9）通讯支持Wifi热点、蓝牙传输，支持自定义数据导入导出,并建立自定义模板，支持导出htf、txt、csv、dat、dxf、gsi、gt7数据格式\n"]
["合计"]